{"text_format":"2","workbook":"xls","n_sheets":4,"sheets":["Sheet1","Sheet2","Sheet3","Sheet4"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":79,"n_cols":5,"rows_kept":79,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["General 967e connection list",null,null," ","2749-01-08"]
[]
[]
[null,"PIN No",null,"DESIGNATION","NOTE"]
[]
[null,1,null,"FUEL TRIM","Mapping Plug 06"]
[null,2,null,"WATER TEMPERATURE SIGNAL"]
[null,3,null,"AIR TEMPERATURE SIGNAL"]
[null,4,null,"5V ANALOGUE","Mapping Plug 04"]
[null,5,null,"ANALOGUE GROUND","Mapping Plug 05"]
[null,6,null,"POWER GROUND","Mapping Plug 01"]
[null,7,null,"POWER GROUND"]
[null,8,null,"POWER GROUND"]
[null,9,null,"POWER GROUND"]
[null,10,null,"GEAR INPUT"]
[null,11,null,"CRANK RETURN"]
[null,12,null,"CRANK SIGNAL"]
[null,13,null,"ECU SUPPLY"]
[null,14,null,"SERIAL RECEIVE","Mapping Plug 03"]
[null,15,null,"FAULT LIGHT / SWITCH"]
[null,16,null,"SHIFT LIGHT","Switched Ground"]
[null,17,null,"FUEL PUMP RELAY DRIVE","Switched Ground"]
[null,18,null,"IGNITION DRIVE 2","Cylinders 2 + 3"]
[null,19,null,"POWERSHIFT INPUT","Ground Active"]
[null,20,null,"THROTTLE SIGNAL"]
[null,21,null,"MAP SIGNAL"," "]
[null,22,null,"5V ANALOGUE"," "]
[null,23,null,"ANALOGUE GROUND"," "]
[null,24,null,"ANALOGUE GROUND"," "]
[null,25,null,"OIL TEMPERATURE"]
[null,26,null,"IGNITION TRIM","Mapping Plug 07"]
[null,27,null,"OIL PRESSURE"]
[null,28,null,"BAROMETRIC PRESSURE SIGNAL / LAUNCH INPUT"]
[null,29,null,"LAMBDA SIGNAL"]
[null,30,null,"NOT USED","Not Used"]
[null,31,null,"NOT USED","Not Used"]
[null,32,null,"SERIAL TRANSMIT","Mapping Plug 02"]
[null,33,null,"RADIATOR FAN RELAY DRIVE","Switched Ground"]
[null,34,null,"TACHOMETER SIGNAL"]
[null,35,null,"INJECTOR OUTPUT","All Cylinders"]
[null,36,null,"IGNITION DRIVE 1","Cylinders 1+ 4 (Coil if distributor fitted)"]
[]
[]
["NOTES:"]
[]
[1,"All digital outputs are switched ground . I.e. to turn on the Shift Light, the ECU output is switched to ground"]
[null,"These type of outputs are on pins: 16, 17 and 33",null,"are on pins 15, 16, 17 and 33"]
[2,"The Mapping Plug should be wired as follows:"]
[null,"ECU Pin #","Mapping Plug Pin #"]
[null,6,1]
[null,32,2]
[null,14,3]
[null,4,4]
[null,5,5]
[null,1,6]
[null,26,7]
[3,"The Powershift input should be switched to ground to activate the Powershift function"]
[4,"The Vauxhall Crankshaft Sensor should be wired as follows:"]
[null,"Sensor #","ECU Pin #"]
[null,1,11]
[null,2,12]
[null,3,"Ground"]
[5,"The Throttle Position Sensor (TPS) should be wired as follows:"]
[null,"Sensor #","ECU Pin #"]
[null,1,"TBA"]
[null,2,"TBA"]
[null,3,"TBA"]
[6,"The Barometric Pressure Sensor should be wired as follows:"]
[null,"Sensor #","ECU Pin #"]
[null,"A",23]
[null,"B",28,"AND LAUNCH INPUT (ground active)"]
[null,"C",22]
[7,"The Lambda Sensor should be wired as follows:"]
[null,"Sensor #","ECU Pin #"]
[null,1,"TBA"]
[null,2,"TBA"]
[null,3,"TBA"]
[null,4,"TBA"]
[8,"The Fault Lamp output is a switched ground"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet4","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}