{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Sheet1 (2)"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1 (2)","index":0,"n_rows":145,"n_cols":5,"rows_kept":145,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["9A6 Pin #","9A6","Electrical Detail A","Electrical Detail B","Notes"]
[" "]
["A001","Ground",null,"GND"]
["A002","Ground",null,"GND"]
["A003","ECU Permanent 12V Supply",null,"12V MEM"]
["A004","12V Switch",null,"12V Key"]
["A005","12V Switch",null,"12V Key"]
["A006","Air Charge Pump Relay",null,"1A LSD"]
["A007","Oil Temp","1k Pull Up","AN"]
["A008","Injector A+",null,"GDI HS"]
["A009","Anti Lag Signal","100k Pull Up","AN"]
["A010","Baro Signal","100k Pull Down","AN"]
["A011","5Va2",null,"5Va"]
["A012","Injector A-",null,"GDI LS"]
["A013","Narrow Band Oxygen Sensor 1","2M2 Pull Down","AN","Use any 0Va for N/Band Oxygen sensor Return"]
["A014","5Va1",null,"5Va"]
["A015","Lambda1 R ",null,"WRL"]
["A016","Cam Return",null,"0V"]
["A017","EGT Signal","100K Pull Up","AN"]
["A018","Air Temp Signal","1k Pull Up","AN"]
["A019",null,"100r Pull Up","AN"]
["A020","0Va",null,"0V"]
["A021",null,null,"1A LSD PWM"]
["A022","Wastegate Drive","1k Pull Up","3A LSD PWM"]
["A023","PWM Water Pump",null,"3A LSD PWM"]
["A024",null,null,"1A LSD PWM"]
["A025","Shift Up Solenoid",null,"1A LSD"]
["A026","Launch Signal","100k Pull Up","AN"]
["A027","Injector C+",null,"GDI HS"]
["A028","Engine Oil Pressure","1k Pull Up","AN"]
["A029","Lambda1 N",null,"WRL"]
["A030","5Va2",null,"5Va"]
["A031","Injector C-",null,"GDI LS"]
["A032","AC Request","100k Pull Down","AN"]
["A033","5Va1",null,"5Va"]
["A034","HP Fuel Signal","100k Pull Up","AN"]
["A035","Cam Supply",null,"5Va"]
["A036","Shift Up","100k Pull Up","AN"]
["A037","Start Request","100k Pull Down","AN"]
["A038","TPS2 Signal ","100k Pull Up","AN"]
["A039","0Va",null,"0V"]
["A040","Egas2 Motor Drive -",null,"H Bridge -"]
["A041","Egas2 Motor Drive +",null,"H Bridge +"]
["A042","Lambda Sensor 2 Heater",null,"5A LSD PWM"]
["A043","Lambda Sensor 1 Heater",null,"5A LSD PWM"]
["A044","Shift Down Solenoid",null,"1A LSD"]
["A045","Pedal A Signal","100k Pull Up","AN"]
["A046","Injector B+",null,"GDI HS"]
["A047","TPS1 Signal ","100k Pull Up","AN"]
["A048","Lambda1 VG",null,"WRL"]
["A049","Lambda1 P",null,"WRL"]
["A050","Injector B-",null,"GDI LS"]
["A051","Engine Stop Signal","100k Pull Down","AN"]
["A052","5Va1",null,"5Va"]
["A053","Gearbox Signal","100k Pull Up","AN"]
["A054","Cam 2Signal","4k7 Pull Up","Cam"]
["A055","Pedal B Signal","100k Pull Down","AN"]
["A056",null,"100k Pull Down","AN"]
["A057","TPS4 Signal ","100k Pull Up","AN"]
["A058","0Va",null,"0V"]
["A059","Egas1 Motor Drive -",null,"H Bridge -"]
["A060","Egas1 Motor Drive +",null,"H Bridge +"]
["A061","HP Fuel Pump Drive",null,"5A peak and hold"]
["A062","Shift Down","100k Pull Up","AN"]
["A063","Rad Fan 1 Relay",null,"1A LSD"]
["A064","Air Accumulator Pressure","100k Pull Down","AN"]
["A065","Injector D+",null,"GDI HS"]
["A066","MAP","100k Pull Down","AN"]
["A067","Water Temp Signal","1k/18k Pull Up","AN"]
["A068","LP Fuel Signal","18k Pull Up","AN"]
["A069","Injector D-",null,"GDI LS"]
["A070","Boost Limit","100k Pull Up","AN"]
["A071","5Va1",null,"5Va"]
["A072","Neutral Request","100k Pull Up","AN"]
["A073","Cam1 Signal","4k7 Pull Up","Cam"]
["A074","TPS3 Signal ","100k Pull Up","AN"]
["A075","Clutch Voltage","100k Pull Up","AN"]
["A076","Nitrous Input Pin","100k Pull Up","AN"]
["A077","0Va",null,"0V"]
["A078",null,null,"1A LSD PWM"]
["A079","Inlet Cam Drive (Cam 1)",null,"3A LSD PWM"]
["A080","Exhaust Cam Drive (Cam 2)",null,"3A LSD PWM"]
["A081","Tachometer Drive",null,"1A LSD PWM"]
[]
[]
[]
["B082","MIL",null,"1A LSD"]
["B083","5Va2",null,"5Va"]
["B084","WS3+","4k7 Pull Up","WS"]
["B085","Knock1 Signal",null,"Knock Sig"]
["B086","WS1+","4k7 Pull Up","WS"]
["B087","MAF Signal","1k2 Pull Up","PWM SIG"]
["B088","CAN2 H",null,"CAN"]
["B089","CAN H",null,"CAN"]
["B090","Fuel Pump Relay",null,"1A LSD"]
["B091","5Va2",null,"5Va"]
["B092","WS4+","4k7 Pull Up","WS"]
["B093","Knock1 Return",null,"Knock Rtn"]
["B094","WS2+","4k7 Pull Up","WS"]
["B095","PWM Pedal","1k2 Pull Up","PWM SIG"]
["B096","CAN2 L",null,"CAN"]
["B097","CAN L",null,"CAN"]
["B098","Engine Stop Output",null,"1A LSD"]
["B099","5Va1",null,"5Va"]
["B100","Crank Signal",null,"Crank","Suggested Raychem Type 44 Screened Cable"]
["B101","Knock 2 Signal",null,"Knock Sig"]
["B102","WS1 Return",null,"0Va"]
["B103","WS2 Return",null,"0Va"]
["B104","WS3 Return",null,"0Va"]
["B105","WS4 Return",null,"0Va"]
["B106","PWR Hold Relay",null,"1A LSD"]
["B107","5Va1",null,"5Va"]
["B108","Crank Return",null,"Crank","Suggested Raychem Type 44 Screened Cable"]
["B109","Knock 2 Return",null,"Knock Rtn"]
["B110","Ignition Drive A",null,"IGN"]
["B111","Ignition Drive B",null,"IGN"]
["B112","Ignition Drive C",null,"IGN"]
["B113","Ignition Drive D",null,"IGN"]
["B114","HSD Battery +",null,"HSD Battery +"]
["B115","HSD Battery +",null,"HSD Battery +"]
["B116","Starter Solenoid Drive",null,"10A HSD"]
["B117","Ignition Output HSD",null,"10A HSD PWM"]
["B118","Rad Fan 1 HSD",null,"10A HSD PWM"]
["B119","n/c",null,"n/c"]
["B120","Fuel Pump HSD",null,"10A HSD PWM"]
["B121","n/c",null,"n/c"]
[" "]
[" "]
[" "]
[" "]
{"$rows_empty":11}
[" "]
[" "]
[" "]
[" "]