{"text_format":"2","workbook":"xls","n_sheets":2,"sheets":["36-1 1-3-4-2 WS","60-2 1-3-4-2 COP"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"36-1 1-3-4-2 WS","index":0,"n_rows":43,"n_cols":4,"rows_kept":43,"cut":false,"hidden":false,"merged":[[0,1,0,3]],"flags":["formulas_cached_only"]}
["MBE9A4","36-1 Grouped Zünd 1-3-4-2"]
[]
["PIN","Kabel","Funktion","Zusatz"]
[]
[1]
[2,null,"Water Temp"]
[3,null,"Air Temp"]
[4,null,"(+5V)"]
[5,null,"(0V)"]
[6,null,"Ground"]
[7,null,"Ground"]
[8,null,"CAN Low"]
[9,null,"CAN High"]
[10,null,"Battery 12V"]
[11,null,"Crank Return"]
[12,null,"Crank Signal"]
[13,null,"Switched 12V"]
[14]
[15,null,"Ignition 4","-"]
[16,null,"Output"]
[17,null,"Output","Fuel Pump"]
[18,null,"Ignition 2","Zyl 2+3"]
[19,null,"Input"]
[20,null,"TPS Signal"]
[21,null,"MAP Signal"]
[22,null,"(+5V)"]
[23,null,"(0V)"]
[24,null,"(0V)"]
[25,null,"Input"]
[26]
[27,null,"Input"]
[28,null,"Baro Sense"]
[29,null,"Lambda Input"]
[30,null,"CAM Signal"]
[31,null,"CAM Return"]
[32]
[33,null,"Output"]
[34,null,"Tacho"]
[35,null,"Ignition 3"]
[36,null,"Ignition 1","Zyl 1+4"]
[]
["Out","Shift Light/Rad Fan/Fuel Pump/Rad Fan2 "]
["In","Wheel Speed / Oil Temp / Gear Position / Oil Press / Fuel Press / Launch"]

{"sheet":"60-2 1-3-4-2 COP","index":1,"n_rows":43,"n_cols":4,"rows_kept":43,"cut":false,"hidden":false,"merged":[[0,1,0,3]],"flags":["formulas_cached_only"]}
["MBE9A4","60-2 COP Zünd 1-3-4-2"]
[]
["PIN","Kabel","Funktion","Zusatz"]
[]
[1]
[2,null,"Water Temp"]
[3,null,"Air Temp"]
[4,null,"(+5V)"]
[5,null,"(0V)"]
[6,null,"Ground"]
[7,null,"Ground"]
[8,null,"CAN Low"]
[9,null,"CAN High"]
[10,null,"Battery 12V"]
[11,null,"Crank Return"]
[12,null,"Crank Signal"]
[13,null,"Switched 12V"]
[14]
[15,null,"Ignition 4","Zylinder 2"]
[16,null,"Output"]
[17,null,"Output","Fuel Pump"]
[18,null,"Ignition 2","Zylinder 3"]
[19,null,"Input"]
[20,null,"TPS Signal"]
[21,null,"MAP Signal"]
[22,null,"(+5V)"]
[23,null,"(0V)"]
[24,null,"(0V)"]
[25,null,"Input"]
[26]
[27,null,"Input"]
[28,null,"Baro Sense"]
[29,null,"Lambda Input"]
[30,null,"CAM Signal"]
[31,null,"CAM Return"]
[32]
[33,null,"Output"]
[34,null,"Tacho"]
[35,null,"Ignition 3","Zylinder 4"]
[36,null,"Ignition 1","Zylinder 1"]
[]
["Out","Shift Light/Rad Fan/Fuel Pump/Rad Fan2 "]
["In","Wheel Speed / Oil Temp / Gear Position / Oil Press / Fuel Press / Launch"]