{"text_format":"2","workbook":"xls","n_sheets":9,"sheets":["DIS BMW 1-5-3-6-2-4","COP 1-2-4-3","COP Zünd 1-3-4-2","WS Zünd 1-3-4-2 ","COP V6 Audi 1-4-3-6-2-5","COP BMW 1-5-3-6-2-4","V8 Audi 1-5-4-8-6-3-7-2","V8 Rover 1–8-4-3-6-5-7-2","V8 BMW 1-5-4-8-7-2-6-3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"DIS BMW 1-5-3-6-2-4","index":0,"n_rows":40,"n_cols":4,"rows_kept":40,"cut":false,"hidden":false,"merged":[[0,1,0,3]],"flags":["formulas_cached_only"]}
["MBE 9A8","DIS BMW 1-5-3-6-2-4"]
[]
["PIN","Kabel","Funktion","Zusatz"]
[]
[1,null,"Injektor 4","Zylinder 6"]
[2,null,"Water Temp"]
[3,null,"Air Temp"]
[4,null,"(+5V)"]
[5,null,"(0V)"]
[6,null,"Ground"]
[7,null,"Ground"]
[8,null,"CAN Low"]
[9,null,"CAN High"]
[10,null,"Battery 12V"]
[11,null,"Crank Return"]
[12,null,"Crank Signal"]
[13,null,"Battery/Ign 12V"]
[14,null,"Injektor 1","Zylinder 1"]
[15,null,"Ignition 4"]
[16,null,"Output","ShiftLight"]
[17,null,"Output","Fuel Pump"]
[18,null,"Ignition 2","COIL"]
[19,null,"Input","PowerShift"]
[20,null,"TPS Signal"]
[21,null,"MAP Signal"]
[22,null,"Injektor 5","Zylinder 2"]
[23,null,"Injektor 6","Zylinder 4"]
[24,null,"Injektor 7"]
[25,null,"Input"]
[26,null,"Injektor 3","Zylinder 3"]
[27,null,"Input","LA2"]
[28,null,"Baro Sense"]
[29,null,"Lambda Input"]
[30,null,"CAM Signal"]
[31,null,"Injektor 8"]
[32,null,"Injektor 2","Zylinder 5"]
[33,null,"Output","RadFan, Wastegate!"]
[34,null,"Output","Tacho"]
[35,null,"Ignition 3","COIL"]
[36,null,"Ignition 1","COIL"]

{"sheet":"COP 1-2-4-3","index":1,"n_rows":40,"n_cols":4,"rows_kept":40,"cut":false,"hidden":false,"merged":[[0,1,0,3]],"flags":["formulas_cached_only"]}
["MBE 9A8","COP Zünd 1-2-4-3"]
["Hayabusa MK8"]
["PIN","Kabel","Funktion","Zusatz"]
[]
[1,null,"Injektor 4","unten Zyl 3"]
[2,null,"Water Temp"]
[3,null,"Air Temp"]
[4,null,"(+5V)"]
[5,null,"(0V)"]
[6,null,"Ground"]
[7,null,"Ground"]
[8,"gr","CAN Low"]
[9,"ws","CAN High"]
[10,null,"Battery/Ign 12V"]
[11,null,"Crank Return"]
[12,null,"Crank Signal"]
[13,null,"IGN 12V"]
[14,null,"Injektor 1","unten Zyl 1"]
[15,null,"Ignition 4","Zylinder 3"]
[16,null,"Output","ShiftLight"]
[17,null,"Output","Fuel Pump"]
[18,null,"Ignition 2","Zylinder 2"]
[19,null,"Input"]
[20,null,"TPS Signal"]
[21,null,"MAP Signal"]
[22,null,"Injektor 5","oben Zyl 1"]
[23,null,"Injektor 6","oben Zyl 2"]
[24,null,"Injektor 7","oben Zyl 4"]
[25,null,"Input"]
[26,null,"Injektor 3","unten Zyl 4"]
[27,null,"Input"]
[28,null,"Baro Sense"]
[29,null,"Lambda Input"]
[30,null,"CAM Signal"]
[31,null,"Injektor 8","oben Zyl 3"]
[32,null,"Injektor 2","unten Zyl 2"]
[33,null,"Output","RadFan, Wastegate!"]
[34,null,"Output","Tacho"]
[35,null,"Ignition 3","Zylinder 4"]
[36,null,"Ignition 1","Zylinder 1"]

{"sheet":"COP Zünd 1-3-4-2","index":2,"n_rows":40,"n_cols":4,"rows_kept":40,"cut":false,"hidden":false,"merged":[[0,1,0,3]],"flags":["formulas_cached_only"]}
["MBE 9A8","COP Zünd 1-3-4-2"]
[]
["PIN","Kabel","Funktion","Zusatz"]
[]
[1,null,"Injektor 4","unten Zyl 2"]
[2,null,"Water Temp"]
[3,null,"Air Temp"]
[4,null,"(+5V)"]
[5,null,"(0V)"]
[6,null,"Ground"]
[7,null,"Ground"]
[8,"gr","CAN Low"]
[9,"ws","CAN High"]
[10,null,"Battery 12V"]
[11,"br","Crank Return"]
[12,"ws","Crank Signal"]
[13,null,"Battery/Ign 12V"]
[14,null,"Injektor 1","unten Zyl 1"]
[15,null,"Ignition 4","Zylinder 2"]
[16,null,"Output","ShiftLight"]
[17,null,"Output","Fuel Pump"]
[18,null,"Ignition 2","Zylinder 3"]
[19,null,"Input"]
[20,null,"TPS Signal"]
[21,null,"MAP Signal"]
[22,null,"Injektor 5","oben Zyl 1"]
[23,null,"Injektor 6","oben Zyl 3"]
[24,null,"Injektor 7","oben Zyl 4"]
[25,null,"Input"]
[26,null,"Injektor 3","unten Zyl 4"]
[27,null,"Input"]
[28,null,"Baro Sense"]
[29,null,"Lambda Input"]
[30,null,"CAM Signal"]
[31,null,"Injektor 8","oben Zyl 2"]
[32,null,"Injektor 2","unten Zyl 3"]
[33,null,"Output","RadFan, Wastegate!"]
[34,null,"Output","Tacho"]
[35,null,"Ignition 3","Zylinder 4"]
[36,null,"Ignition 1","Zylinder 1"]

{"sheet":"WS Zünd 1-3-4-2 ","index":3,"n_rows":40,"n_cols":4,"rows_kept":40,"cut":false,"hidden":false,"merged":[[0,1,0,3]],"flags":["formulas_cached_only"]}
["MBE 9A8","W/S Zünd 1-3-4-2"]
[]
["PIN","Kabel","Funktion","Zusatz"]
[]
[1,null,"Injektor 4","unten Zyl 2"]
[2,null,"Water Temp"]
[3,null,"Air Temp"]
[4,null,"(+5V)"]
[5,null,"(0V)"]
[6,null,"Ground"]
[7,null,"Ground"]
[8,"gr","CAN Low"]
[9,"ws","CAN High"]
[10,null,"Battery 12V"]
[11,"br","Crank Return"]
[12,"ws","Crank Signal"]
[13,null,"Battery/Ign 12V"]
[14,null,"Injektor 1","unten Zyl 1"]
[15,null,"Ignition 4"]
[16,null,"Output","ShiftLight"]
[17,null,"Output","Fuel Pump"]
[18,null,"Ignition 2","Zylinder 3+4"]
[19,null,"Input"]
[20,null,"TPS Signal"]
[21,null,"MAP Signal"]
[22,null,"Injektor 5","oben Zyl 1"]
[23,null,"Injektor 6","oben Zyl 3"]
[24,null,"Injektor 7","oben Zyl 4"]
[25,null,"Input"]
[26,null,"Injektor 3","unten Zyl 4"]
[27,null,"Input"]
[28,null,"Baro Sense"]
[29,null,"Lambda Input"]
[30,null,"CAM Signal"]
[31,null,"Injektor 8","oben Zyl 2"]
[32,null,"Injektor 2","unten Zyl 3"]
[33,null,"Output","RadFan, Wastegate!"]
[34,null,"Output","Tacho"]
[35,null,"Ignition 3"]
[36,null,"Ignition 1","Zylinder 1+2"]

{"sheet":"COP V6 Audi 1-4-3-6-2-5","index":4,"n_rows":40,"n_cols":5,"rows_kept":40,"cut":false,"hidden":false,"merged":[[0,1,0,3]],"flags":["formulas_cached_only"]}
["MBE 9A8","COP Zünd 1-4-3-6-2-5"]
["Audi V6"]
["PIN","Kabel","Funktion","Zusatz"]
[]
[1,null,"Injektor 4","Zylinder 6","LA2"]
[2,null,"Water Temp"]
[3,null,"Air Temp"]
[4,null,"(+5V)"]
[5,null,"(0V)"]
[6,null,"Ground"]
[7,null,"Ground"]
[8,"gr","CAN Low"]
[9,"ws","CAN High"]
[10,null,"Battery 12V"]
[11,"br","Crank Return"]
[12,"ws","Crank Signal"]
[13,null,"Battery/Ign 12V"]
[14,null,"Injektor 1","Zylinder 1","LA1"]
[15,null,"Ignition 4"]
[16,null,"Output","ShiftLight"]
[17,null,"Output","Fuel Pump"]
[18,null,"Ignition 2","Zyl 5/2"]
[19,null,"Input","PowerShift"]
[20,null,"TPS Signal"]
[21,null,"MAP Signal"]
[22,null,"Injektor 5","Zylinder 2","LA1"]
[23,null,"Injektor 6","Zylinder 5","LA2"]
[24,null,"Injektor 7"]
[25,null,"Input"]
[26,null,"Injektor 3","Zylinder 3","LA1"]
[27,null,"Input","LA2"]
[28,null,"Baro Sense"]
[29,null,"Lambda Input"]
[30,null,"CAM Signal"]
[31,null,"Injektor 8"]
[32,null,"Injektor 2","Zylinder 4","LA2"]
[33,null,"Output","RadFan, Wastegate!"]
[34,null,"Output","Tacho"]
[35,null,"Ignition 3","Zyl 3/4"]
[36,null,"Ignition 1","Zyl 1/6"]

{"sheet":"COP BMW 1-5-3-6-2-4","index":5,"n_rows":40,"n_cols":5,"rows_kept":40,"cut":false,"hidden":false,"merged":[[0,1,0,3]],"flags":["formulas_cached_only"]}
["MBE 9A8","COP BMW 1-5-3-6-2-4"]
[]
["PIN","Kabel","Funktion","Zusatz"]
[]
[1,null,"Injektor 4","Zylinder 6","LA2"]
[2,null,"Water Temp"]
[3,null,"Air Temp"]
[4,null,"(+5V)"]
[5,null,"(0V)"]
[6,null,"Ground"]
[7,null,"Ground"]
[8,"gr","CAN Low"]
[9,"ws","CAN High"]
[10,null,"Battery 12V"]
[11,"br","Crank Return"]
[12,"ws","Crank Signal"]
[13,null,"Battery/Ign 12V"]
[14,null,"Injektor 1","Zylinder 1","LA1"]
[15,null,"Ignition 4"]
[16,null,"Output","ShiftLight"]
[17,null,"Output","Fuel Pump"]
[18,null,"Ignition 2","Zyl 5/2"]
[19,null,"Input","PowerShift"]
[20,null,"TPS Signal"]
[21,null,"MAP Signal"]
[22,null,"Injektor 5","Zylinder 2","LA1"]
[23,null,"Injektor 6","Zylinder 4","LA2"]
[24,null,"Injektor 7"]
[25,null,"Input"]
[26,null,"Injektor 3","Zylinder 3","LA1"]
[27,null,"Input","LA2"]
[28,null,"Baro Sense"]
[29,null,"Lambda Input"]
[30,null,"CAM Signal"]
[31,null,"Injektor 8"]
[32,null,"Injektor 2","Zylinder 5","LA2"]
[33,null,"Output","RadFan, Wastegate!"]
[34,null,"Output","Tacho"]
[35,null,"Ignition 3","Zyl 3/4"]
[36,null,"Ignition 1","Zyl 1/6"]

{"sheet":"V8 Audi 1-5-4-8-6-3-7-2","index":6,"n_rows":47,"n_cols":5,"rows_kept":47,"cut":false,"hidden":false,"merged":[[0,1,0,3]],"flags":["formulas_cached_only"]}
["MBE 9A8","COP Zünd 1-5-4-8-6-3-7-2"]
["Audi V8","Offset -450°"]
["PIN","Kabel","Funktion","Zusatz"]
[]
[1,null,"Injektor 4","Zylinder 1","LA1"]
[2,null,"Water Temp"]
[3,null,"Air Temp"]
[4,null,"(+5V)"]
[5,null,"(0V)"]
[6,null,"Ground"]
[7,null,"Ground"]
[8,"gr","CAN Low"]
[9,"ws","CAN High"]
[10,null,"Battery 12V"]
[11,"br","Crank Return"]
[12,"ws","Crank Signal"]
[13,null,"Battery/Ign 12V"]
[14,null,"Injektor 1","Zylinder 3","LA1"]
[15,null,"Ignition 4","Zyl 1/6"]
[16,null,"Output"]
[17,null,"Output","Fuel Pump"]
[18,null,"Ignition 2","Zyl 4/7"]
[19,null,"Input"]
[20,null,"TPS Signal"]
[21,null,"MAP Signal"]
[22,null,"Injektor 5","Zylinder 5","LA2"]
[23,null,"Injektor 6","Zylinder 4","LA1"]
[24,null,"Injektor 7","Zylinder 8","LA2"]
[25,null,"Input"]
[26,null,"Injektor 3","Zylinder 2","LA1"]
[27,null,"Input","Lambda 2"]
[28,null,"Baro Sense","Baro & PowerShift"]
[29,null,"Lambda Input"]
[30,null,"CAM Signal"]
[31,null,"Injektor 8","Zylinder 6","LA2 "]
[32,null,"Injektor 2","Zylinder 7","LA2"]
[33,null,"Output","RadFan, Wastegate!"]
[34,null,"Output","Tacho"]
[35,null,"Ignition 3","Zyl 8/2"]
[36,null,"Ignition 1","Zyl 3/5"]
[]
[]
[null,null,"Cylinder orientation"]
[null,null,1,5]
[null,null,2,6]
[null,null,3,7]
[null,null,4,8]

{"sheet":"V8 Rover 1–8-4-3-6-5-7-2","index":7,"n_rows":47,"n_cols":5,"rows_kept":47,"cut":false,"hidden":false,"merged":[[0,1,0,3]],"flags":["formulas_cached_only"]}
["MBE 9A8","COP Zünd 1–8-4-3-6-5-7-2"]
["Rover","Offset -450°"]
["PIN","Kabel","Funktion","Zusatz"]
[]
[1,null,"Injektor 4","Zylinder 7","LA1"]
[2,null,"Water Temp"]
[3,null,"Air Temp"]
[4,null,"(+5V)"]
[5,null,"(0V)"]
[6,null,"Ground"]
[7,null,"Ground"]
[8,"gr","CAN Low"]
[9,"ge","CAN High"]
[10,null,"Battery 12V"]
[11,"br","Crank Return"]
[12,"ws","Crank Signal"]
[13,null,"Battery/Ign 12V"]
[14,null,"Injektor 1","Zylinder 3","LA1"]
[15,null,"Ignition 4","Zyl 4/7"]
[16,null,"Output"]
[17,null,"Output","Fuel Pump"]
[18,null,"Ignition 2","Zyl 1/6"]
[19,null,"Input"]
[20,null,"TPS Signal"]
[21,null,"MAP Signal"]
[22,null,"Injektor 5","Zylinder 2","LA2"]
[23,null,"Injektor 6","Zylinder 1","LA1"]
[24,null,"Injektor 7","Zylinder 8","LA2"]
[25,null,"Input"]
[26,null,"Injektor 3","Zylinder 5","LA1"]
[27,null,"Input","Lambda 2"]
[28,null,"Baro Sense","Baro & PowerShift"]
[29,null,"Lambda Input"]
[30,null,"CAM Signal"]
[31,null,"Injektor 8","Zylinder 4","LA2 "]
[32,null,"Injektor 2","Zylinder 6","LA2"]
[33,null,"Output","RadFan, Wastegate!"]
[34,null,"Output","Tacho"]
[35,null,"Ignition 3","Zyl 8/5"]
[36,null,"Ignition 1","Zyl 3/2"]
[]
[]
[null,null,"Cylinder orientation"]
[null,null,1,2]
[null,null,3,4]
[null,null,5,6]
[null,null,7,8]

{"sheet":"V8 BMW 1-5-4-8-7-2-6-3","index":8,"n_rows":47,"n_cols":5,"rows_kept":47,"cut":false,"hidden":false,"merged":[[0,1,0,3]],"flags":["formulas_cached_only"]}
["MBE 9A8","COP Zünd 1-5-4-8-7-2-6-3"]
["BMW S65 V8","Offset beachten! -450°"]
["PIN","Kabel","Funktion","Zusatz"]
[]
[1,null,"Injektor 4","Zylinder 1","LA1"]
[2,null,"Water Temp"]
[3,null,"Air Temp"]
[4,null,"(+5V)"]
[5,null,"(0V)"]
[6,null,"Ground"]
[7,null,"Ground"]
[8,"gr","CAN Low"]
[9,"ws","CAN High"]
[10,null,"Battery 12V"]
[11,"br","Crank Return"]
[12,"ws","Crank Signal"]
[13,null,"Battery/Ign 12V"]
[14,null,"Injektor 1","Zylinder 2","LA1"]
[15,null,"Ignition 4","Zyl 1/7"]
[16,null,"Output"]
[17,null,"Output","Fuel Pump"]
[18,null,"Ignition 2","Zyl 4/6"]
[19,null,"Input"]
[20,null,"TPS Signal"]
[21,null,"MAP Signal"]
[22,null,"Injektor 5","Zylinder 5","LA2"]
[23,null,"Injektor 6","Zylinder 4","LA1"]
[24,null,"Injektor 7","Zylinder 8","LA2"]
[25,null,"Input"]
[26,null,"Injektor 3","Zylinder 3","LA1"]
[27,null,"Input","Lambda 2"]
[28,null,"Baro Sense","Baro & PowerShift"]
[29,null,"Lambda Input"]
[30,null,"CAM Signal"]
[31,null,"Injektor 8","Zylinder 7","LA2 "]
[32,null,"Injektor 2","Zylinder 6","LA2"]
[33,null,"Output","RadFan, Wastegate!"]
[34,null,"Output","Tacho"]
[35,null,"Ignition 3","Zyl 8/3"]
[36,null,"Ignition 1","Zyl 5/2"]
[]
[]
[null,null,"Cylinder orientation"]
[null,null,5,1]
[null,null,6,2]
[null,null,7,3]
[null,null,8,4]