{"text_format":"2","workbook":"xls","n_sheets":8,"sheets":["BMW 6Zyl","4Zyl1342 upper","4Zyl1342","Ford V8","BMW V8","Audi I5","BMW V8 VANOS","Audi V8"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"BMW 6Zyl","index":0,"n_rows":126,"n_cols":5,"rows_kept":126,"cut":false,"hidden":false,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["MBE 9A9"]
["BMW 6Zyl 1-5-3-6-2-4"]
[]
["A001",null,"Ground","GND"]
["A002",null,"Ground","GND"]
["A003",null,"ECU Permanent 12V Supply","12V MEM"]
["A004",null,"12V Switch","12V Key"]
["A005",null,"12V Switch","12V Key"]
["A006",null,"Air Charge Pump Relay","1A LSD"]
["A007",null,"Oil Temp","1k Pull Up"]
["A008",null,"Injector Drive D","1A LSD","Zyl 6"]
["A009",null,"Anti Lag Signal","100k Pull Up"]
["A010",null,"Baro Signal","100k Pull Down"]
["A011",null,"5Va2","5Va2"]
["A012",null,"Injector Drive H","1A LSD"]
["A013",null,"Narrow Band Oxygen Sensor 1","2M2 Pull Down"]
["A014",null,"Rad Fan Relay 2","1A LSD"]
["A015",null,"Lambda1 R "]
["A016",null,"Cam Return","0V"]
["A017",null,"EGT Signal","100k Pull Up"]
["A018",null,"Air Temp Signal","1k Pull Up"]
["A019",null,"Engine Oil Pressure Signal","100r Pull Up"]
["A020",null,"Shift Up Solenoid","1A LSD"]
["A021",null,"Ignition Drive E",null,"Zylinder 2"]
["A022",null,"Ignition Drive F",null,"Zylinder 4"]
["A023",null,"Ignition Drive G"]
["A024",null,"Ignition Drive H"]
["A025",null,"Shift Light","1A LSD"]
["A026",null,"Launch Signal","100k Pull Up"]
["A027",null,"Injector Drive C","1A LSD","Zyl 3"]
["A028",null,null,"1k Pull Up"]
["A029",null,"Lambda1 N"]
["A030",null,"5Va2","5Va2"]
["A031",null,"Injector Drive G","1A LSD"]
["A032",null,"0va","0Va"]
["A033",null,null,"1A LSD"]
["A034",null,"Fuel Pressure Signal","100r Pull Up"]
["A035",null,"Cam Supply","5Va2"]
["A036",null,"MAP 2 Signal","100k Pull Down"]
["A037",null,"Powershift Signal","100k Pull Up (Digital Only)"]
["A038",null,"TPS2 Signal","100k Pull Up"]
["A039",null,null,"1A LSD"]
["A040",null,"Egas2 Motor Drive -","H Bridge"]
["A041",null,"Egas2 Motor Drive +","H Bridge"]
["A042",null,"Lambda Sensor 2 Heater","5A LS PWM"]
["A043",null,"Lambda Sensor 1 Heater","5A LS PWM"]
["A044",null,"Shift Light 2","1A LSD"]
["A045",null,"Pedal A Signal","100k Pull Up"]
["A046",null,"Injector Drive B","1A LSD","Zyl 5"]
["A047",null,"TPS1 Signal ","100k Pull Up"]
["A048",null,"Lambda1 VG"]
["A049",null,"Lambda1 P"]
["A050",null,"Injector Drive E","1A LSD","Zyl 2"]
["A051",null,"0Va","0Va"]
["A052",null,"Rad Fan Relay 1","1A LSD"]
["A053",null,"Gearbox Signal","100k Pull Up"]
["A054",null,"Cam 2 Signal","4k7 Pull Up"]
["A055",null,"Pedal B Signal","100k Pull Down"]
["A056",null,"Engine Stop Signal","100k Pull Down"]
["A057",null,"TPS4 Signal ","100k Pull Up"]
["A058",null,"Down Shift Solenoid","1A LSD"]
["A059",null,"Egas1 Motor Drive -","H Bridge"]
["A060",null,"Egas1 Motor Drive +","H Bridge"]
["A061",null,"Varable Cam 2 Drive","2A LSD PWM"]
["A062",null,"Varable Cam 1 Drive","2A LSD PWM"]
["A063",null,"Neutral Light","1A LSD"]
["A064",null,null,"1k Pull Up"]
["A065",null,"Injector Drive A","1A LSD","Zyl 1"]
["A066",null,"MAP Signal","100k Pull Down"]
["A067",null,"Water Temp Signal","1k/18k Pull Up"]
["A068",null,"Neutral Request","18k Pull Up"]
["A069",null,"Injector Drive F","1A LSD","Zyl 4"]
["A070",null,"0Va","0Va"]
["A071",null,"Throttle Blip Solenoid","1A LSD"]
["A072",null,"Narrow Band Oxygen Sensor 2","2M2 Pull Down"]
["A073",null,"Cam1 Signal","4k7 Pull Up"]
["A074",null,"TPS3 Signal ","100K Pull up"]
["A075",null,"AirPressure Input","100k Pull Down"]
["A076",null,"Nitrous Input Pin","100k Pull Up"]
["A077",null,null,"1A LSD"]
["A078",null,null,"0.5A LSD PWM"]
["A079",null,"Wastegate Drive","2A LSD PWM"]
["A080",null,"PWM Water Pump","2A LSD PWM"]
["A081",null,"Tachometer Drive","0.5A LSD PWM 1k Pull Up"]
[]
["B082",null,null,"1A LSD"]
["B083",null,"Lambda2 P"]
["B084",null,"Lambda2 R"]
["B085",null,"Knock1 Signal"]
["B086",null,"Wheelspeed 1 (FL)","4k7 Pull Up"]
["B087",null,"Wheelspeed 2 (FR)","4k7 Pull Up"]
["B088",null,"Serial TXD / CAN 2 H"]
["B089",null,"CAN H"]
["B090",null,"Fuel Pump Relay","1A LSD"]
["B091",null,"Lambda2 N"]
["B092",null,"Lambda2 VG"]
["B093",null,"Knock1 Return"]
["B094",null,"Wheelspeed 3 (RL)","4k7 Pull Up"]
["B095",null,"Wheelspeed 4 (RR)","4k7 Pull Up"]
["B096",null,"Serial RXD / CAN 2 L"]
["B097",null,"CAN L"]
["B098",null,"Engine Stop Output","1A LSD"]
["B099",null,"5Va1","5Va1"]
["B100",null,"Crank Signal"]
["B101",null,"Knock 2 Signal"]
["B102",null,"WheelSpeed1 Return","0V"]
["B103",null,"WheelSpeed2 Return","0V"]
["B104",null,"WheelSpeed3 Return","0V"]
["B105",null,"WheelSpeed4 Return","0V"]
["B106",null,"PWR Hold Relay","1A LSD"]
["B107",null,"5Va1","5Va1"]
["B108",null,"Crank Return","0V"]
["B109",null,"Knock 2 Return"]
["B110",null,"Ignition Drive A",null,"Zylinder 1"]
["B111",null,"Ignition Drive B",null,"Zylinder 5"]
["B112",null,"Ignition Drive C",null,"Zylinder 3"]
["B113",null,"Ignition Drive D",null,"Zylinder 6"]
["B114",null,"HSD Battery +","12V Perm (HSD Power)"]
["B115",null,"HSD Battery +","12V Perm (HSD Power)"]
["B116",null,"Starter Solenoid","10A HSD PWM"]
["B117",null,"Ignition Output","10A HSD PWM","LA Power"]
["B118",null,"Rad Fan 1 HSD","10A HSD PWM","CAM1 Advanced"]
["B119",null,"Fuel Pump","10A HSD PWM","CAM1 Retard"]
["B120",null,"Engine Stop Output","10A HSD PWM","CAM2 Advanced"]
["B121",null,"PWM Water Pump","10A HSD PWM","CAM2 Retard"]
[" "]

{"sheet":"4Zyl1342 upper","index":1,"n_rows":126,"n_cols":5,"rows_kept":126,"cut":false,"hidden":false,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["MBE 9A9"]
["4Zylinder 8 Injektoren 1-3-4-2"]
[]
["A001",null,"Ground","GND"]
["A002",null,"Ground","GND"]
["A003",null,"ECU Permanent 12V Supply","12V MEM"]
["A004",null,"12V Switch","12V Key"]
["A005",null,"12V Switch","12V Key"]
["A006",null,"Air Charge Pump Relay","1A LSD"]
["A007",null,"Oil Temp","1k Pull Up"]
["A008",null,"Injector Drive D","1A LSD","Zyl 2"]
["A009",null,"Anti Lag Signal","100k Pull Up"]
["A010",null,"Baro Signal","100k Pull Down"]
["A011",null,"5Va2","5Va2"]
["A012",null,"Injector Drive H","1A LSD","Zyl 2 oben"]
["A013",null,"Narrow Band Oxygen Sensor 1","2M2 Pull Down"]
["A014",null,"Rad Fan Relay 2","1A LSD"]
["A015",null,"Lambda1 R "]
["A016",null,"Cam Return","0V"]
["A017",null,"EGT Signal","100k Pull Up"]
["A018",null,"Air Temp Signal","1k Pull Up"]
["A019",null,"Engine Oil Pressure Signal","100r Pull Up"]
["A020",null,"Shift Up Solenoid","1A LSD"]
["A021",null,"Ignition Drive E"]
["A022",null,"Ignition Drive F"]
["A023",null,"Ignition Drive G"]
["A024",null,"Ignition Drive H"]
["A025",null,"Shift Light","1A LSD"]
["A026",null,"Launch Signal","100k Pull Up"]
["A027",null,"Injector Drive C","1A LSD","Zyl 4"]
["A028",null,null,"1k Pull Up"]
["A029",null,"Lambda1 N"]
["A030",null,"5Va2","5Va2"]
["A031",null,"Injector Drive G","1A LSD","Zyl 4 oben"]
["A032",null,"0va","0Va"]
["A033",null,null,"1A LSD"]
["A034",null,"Fuel Pressure Signal","100r Pull Up"]
["A035",null,"Cam Supply","5Va2"]
["A036",null,"MAP 2 Signal","100k Pull Down"]
["A037",null,"Powershift Signal","100k Pull Up (Digital Only)"]
["A038",null,"TPS2 Signal","100k Pull Up"]
["A039",null,null,"1A LSD"]
["A040",null,"Egas2 Motor Drive -","H Bridge"]
["A041",null,"Egas2 Motor Drive +","H Bridge"]
["A042",null,"Lambda Sensor 2 Heater","5A LS PWM"]
["A043",null,"Lambda Sensor 1 Heater","5A LS PWM"]
["A044",null,"Shift Light 2","1A LSD"]
["A045",null,"Pedal A Signal","100k Pull Up"]
["A046",null,"Injector Drive B","1A LSD","Zyl 3"]
["A047",null,"TPS1 Signal ","100k Pull Up"]
["A048",null,"Lambda1 VG"]
["A049",null,"Lambda1 P"]
["A050",null,"Injector Drive E","1A LSD","Zyl 1 oben"]
["A051",null,"0Va","0Va"]
["A052",null,"Rad Fan Relay 1","1A LSD"]
["A053",null,"Gearbox Signal","100k Pull Up"]
["A054",null,"Cam 2 Signal","4k7 Pull Up"]
["A055",null,"Pedal B Signal","100k Pull Down"]
["A056",null,"Engine Stop Signal","100k Pull Down"]
["A057",null,"TPS4 Signal ","100k Pull Up"]
["A058",null,"Down Shift Solenoid","1A LSD"]
["A059",null,"Egas1 Motor Drive -","H Bridge"]
["A060",null,"Egas1 Motor Drive +","H Bridge"]
["A061",null,"Varable Cam 2 Drive","2A LSD PWM"]
["A062",null,"Varable Cam 1 Drive","2A LSD PWM"]
["A063",null,"Neutral Light","1A LSD"]
["A064",null,null,"1k Pull Up"]
["A065",null,"Injector Drive A","1A LSD","Zyl 1"]
["A066",null,"MAP Signal","100k Pull Down"]
["A067",null,"Water Temp Signal","1k/18k Pull Up"]
["A068",null,"Neutral Request","18k Pull Up"]
["A069",null,"Injector Drive F","1A LSD","Zyl 3 oben"]
["A070",null,"0Va","0Va"]
["A071",null,"Throttle Blip Solenoid","1A LSD"]
["A072",null,"Narrow Band Oxygen Sensor 2","2M2 Pull Down"]
["A073",null,"Cam1 Signal","4k7 Pull Up"]
["A074",null,"TPS3 Signal ","100K Pull up"]
["A075",null,"AirPressure Input","100k Pull Down"]
["A076",null,"Nitrous Input Pin","100k Pull Up"]
["A077",null,null,"1A LSD"]
["A078",null,null,"0.5A LSD PWM"]
["A079",null,"Wastegate Drive","2A LSD PWM"]
["A080",null,"PWM Water Pump","2A LSD PWM"]
["A081",null,"Tachometer Drive","0.5A LSD PWM 1k Pull Up"]
[]
["B082",null,null,"1A LSD"]
["B083",null,"Lambda2 P"]
["B084",null,"Lambda2 R"]
["B085",null,"Knock1 Signal"]
["B086",null,"Wheelspeed 1 (FL)","4k7 Pull Up"]
["B087",null,"Wheelspeed 2 (FR)","4k7 Pull Up"]
["B088",null,"Serial TXD / CAN 2 H"]
["B089",null,"CAN H"]
["B090",null,"Fuel Pump Relay","1A LSD"]
["B091",null,"Lambda2 N"]
["B092",null,"Lambda2 VG"]
["B093",null,"Knock1 Return"]
["B094",null,"Wheelspeed 3 (RL)","4k7 Pull Up"]
["B095",null,"Wheelspeed 4 (RR)","4k7 Pull Up"]
["B096",null,"Serial RXD / CAN 2 L"]
["B097",null,"CAN L"]
["B098",null,"Engine Stop Output","1A LSD"]
["B099",null,"5Va1","5Va1"]
["B100",null,"Crank Signal"]
["B101",null,"Knock 2 Signal"]
["B102",null,"WheelSpeed1 Return","0V"]
["B103",null,"WheelSpeed2 Return","0V"]
["B104",null,"WheelSpeed3 Return","0V"]
["B105",null,"WheelSpeed4 Return","0V"]
["B106",null,"PWR Hold Relay","1A LSD"]
["B107",null,"5Va1","5Va1"]
["B108",null,"Crank Return","0V"]
["B109",null,"Knock 2 Return"]
["B110",null,"Ignition Drive A",null,"Zylinder 1"]
["B111",null,"Ignition Drive B",null,"Zylinder 3"]
["B112",null,"Ignition Drive C",null,"Zylinder 4"]
["B113",null,"Ignition Drive D",null,"Zylinder 2"]
["B114",null,"HSD Battery +","12V Perm (HSD Power)"]
["B115",null,"HSD Battery +","12V Perm (HSD Power)"]
["B116",null,"Starter Solenoid","10A HSD PWM"]
["B117",null,"Ignition Output","10A HSD PWM","LA Power"]
["B118",null,"Rad Fan 1 HSD","10A HSD PWM"]
["B119",null,"Fuel Pump","10A HSD PWM"]
["B120",null,"Engine Stop Output","10A HSD PWM"]
["B121",null,"PWM Water Pump","10A HSD PWM"]
[" "]

{"sheet":"4Zyl1342","index":2,"n_rows":126,"n_cols":5,"rows_kept":126,"cut":false,"hidden":false,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["MBE 9A9"]
["4Zylinder 1-3-4-2"]
[]
["A001",null,"Ground","GND"]
["A002",null,"Ground","GND"]
["A003",null,"ECU Permanent 12V Supply","12V MEM"]
["A004",null,"12V Switch","12V Key"]
["A005",null,"12V Switch","12V Key"]
["A006",null,"Air Charge Pump Relay","1A LSD"]
["A007",null,"Oil Temp","1k Pull Up"]
["A008",null,"Injector Drive D","1A LSD","Zyl 2"]
["A009",null,"Anti Lag Signal","100k Pull Up"]
["A010",null,"Baro Signal","100k Pull Down"]
["A011",null,"5Va2","5Va2"]
["A012",null,"Injector Drive H","1A LSD"]
["A013",null,"Narrow Band Oxygen Sensor 1","2M2 Pull Down"]
["A014",null,"Rad Fan Relay 2","1A LSD"]
["A015",null,"Lambda1 R "]
["A016",null,"Cam Return","0V"]
["A017",null,"EGT Signal","100k Pull Up"]
["A018",null,"Air Temp Signal","1k Pull Up"]
["A019",null,"Engine Oil Pressure Signal","100r Pull Up"]
["A020",null,"Shift Up Solenoid","1A LSD"]
["A021",null,"Ignition Drive E"]
["A022",null,"Ignition Drive F"]
["A023",null,"Ignition Drive G"]
["A024",null,"Ignition Drive H"]
["A025",null,"Shift Light","1A LSD"]
["A026",null,"Launch Signal","100k Pull Up"]
["A027",null,"Injector Drive C","1A LSD","Zyl 4"]
["A028",null,null,"1k Pull Up"]
["A029",null,"Lambda1 N"]
["A030",null,"5Va2","5Va2"]
["A031",null,"Injector Drive G","1A LSD"]
["A032",null,"0va","0Va"]
["A033",null,null,"1A LSD"]
["A034",null,"Fuel Pressure Signal","100r Pull Up"]
["A035",null,"Cam Supply","5Va2"]
["A036",null,"MAP 2 Signal","100k Pull Down"]
["A037",null,"Powershift Signal","100k Pull Up (Digital Only)"]
["A038",null,"TPS2 Signal","100k Pull Up"]
["A039",null,null,"1A LSD"]
["A040",null,"Egas2 Motor Drive -","H Bridge"]
["A041",null,"Egas2 Motor Drive +","H Bridge"]
["A042",null,"Lambda Sensor 2 Heater","5A LS PWM"]
["A043",null,"Lambda Sensor 1 Heater","5A LS PWM"]
["A044",null,"Shift Light 2","1A LSD"]
["A045",null,"Pedal A Signal","100k Pull Up"]
["A046",null,"Injector Drive B","1A LSD","Zyl 3"]
["A047",null,"TPS1 Signal ","100k Pull Up"]
["A048",null,"Lambda1 VG"]
["A049",null,"Lambda1 P"]
["A050",null,"Injector Drive E","1A LSD"]
["A051",null,"0Va","0Va"]
["A052",null,"Rad Fan Relay 1","1A LSD"]
["A053",null,"Gearbox Signal","100k Pull Up"]
["A054",null,"Cam 2 Signal","4k7 Pull Up"]
["A055",null,"Pedal B Signal","100k Pull Down"]
["A056",null,"Engine Stop Signal","100k Pull Down"]
["A057",null,"TPS4 Signal ","100k Pull Up"]
["A058",null,"Down Shift Solenoid","1A LSD"]
["A059",null,"Egas1 Motor Drive -","H Bridge"]
["A060",null,"Egas1 Motor Drive +","H Bridge"]
["A061",null,"Varable Cam 2 Drive","2A LSD PWM"]
["A062",null,"Varable Cam 1 Drive","2A LSD PWM"]
["A063",null,"Neutral Light","1A LSD"]
["A064",null,null,"1k Pull Up"]
["A065",null,"Injector Drive A","1A LSD","Zyl 1"]
["A066",null,"MAP Signal","100k Pull Down"]
["A067",null,"Water Temp Signal","1k/18k Pull Up"]
["A068",null,"Neutral Request","18k Pull Up"]
["A069",null,"Injector Drive F","1A LSD"]
["A070",null,"0Va","0Va"]
["A071",null,"Throttle Blip Solenoid","1A LSD"]
["A072",null,"Narrow Band Oxygen Sensor 2","2M2 Pull Down"]
["A073",null,"Cam1 Signal","4k7 Pull Up"]
["A074",null,"TPS3 Signal ","100K Pull up"]
["A075",null,"AirPressure Input","100k Pull Down"]
["A076",null,"Nitrous Input Pin","100k Pull Up"]
["A077",null,null,"1A LSD"]
["A078",null,null,"0.5A LSD PWM"]
["A079",null,"Wastegate Drive","2A LSD PWM"]
["A080",null,"PWM Water Pump","2A LSD PWM"]
["A081",null,"Tachometer Drive","0.5A LSD PWM 1k Pull Up"]
[]
["B082",null,null,"1A LSD"]
["B083",null,"Lambda2 P"]
["B084",null,"Lambda2 R"]
["B085",null,"Knock1 Signal"]
["B086",null,"Wheelspeed 1 (FL)","4k7 Pull Up"]
["B087",null,"Wheelspeed 2 (FR)","4k7 Pull Up"]
["B088",null,"Serial TXD / CAN 2 H"]
["B089",null,"CAN H"]
["B090",null,"Fuel Pump Relay","1A LSD"]
["B091",null,"Lambda2 N"]
["B092",null,"Lambda2 VG"]
["B093",null,"Knock1 Return"]
["B094",null,"Wheelspeed 3 (RL)","4k7 Pull Up"]
["B095",null,"Wheelspeed 4 (RR)","4k7 Pull Up"]
["B096",null,"Serial RXD / CAN 2 L"]
["B097",null,"CAN L"]
["B098",null,"Engine Stop Output","1A LSD"]
["B099",null,"5Va1","5Va1"]
["B100",null,"Crank Signal"]
["B101",null,"Knock 2 Signal"]
["B102",null,"WheelSpeed1 Return","0V"]
["B103",null,"WheelSpeed2 Return","0V"]
["B104",null,"WheelSpeed3 Return","0V"]
["B105",null,"WheelSpeed4 Return","0V"]
["B106",null,"PWR Hold Relay","1A LSD"]
["B107",null,"5Va1","5Va1"]
["B108",null,"Crank Return","0V"]
["B109",null,"Knock 2 Return"]
["B110",null,"Ignition Drive A",null,"Zylinder 1"]
["B111",null,"Ignition Drive B",null,"Zylinder 3"]
["B112",null,"Ignition Drive C",null,"Zylinder 4"]
["B113",null,"Ignition Drive D",null,"Zylinder 2"]
["B114",null,"HSD Battery +","12V Perm (HSD Power)"]
["B115",null,"HSD Battery +","12V Perm (HSD Power)"]
["B116",null,"Starter Solenoid","10A HSD PWM"]
["B117",null,"Ignition Output","10A HSD PWM","LA Power"]
["B118",null,"Rad Fan 1 HSD","10A HSD PWM"]
["B119",null,"Fuel Pump","10A HSD PWM"]
["B120",null,"Engine Stop Output","10A HSD PWM"]
["B121",null,"PWM Water Pump","10A HSD PWM"]
[" "]

{"sheet":"Ford V8","index":3,"n_rows":126,"n_cols":5,"rows_kept":126,"cut":false,"hidden":false,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["MBE 9A9"]
["Ford V8 1-5-4-2-6-3-7-8"]
[]
["A001",null,"Ground","GND"]
["A002",null,"Ground","GND"]
["A003",null,"ECU Permanent 12V Supply","12V MEM"]
["A004",null,"12V Switch","12V Key"]
["A005",null,"12V Switch","12V Key"]
["A006",null,"Air Charge Pump Relay","1A LSD"]
["A007",null,"Oil Temp","1k Pull Up"]
["A008",null,"Injector Drive D","1A LSD","Zyl 2"]
["A009",null,"Anti Lag Signal","100k Pull Up"]
["A010",null,"Baro Signal","100k Pull Down"]
["A011",null,"5Va2","5Va2"]
["A012",null,"Injector Drive H","1A LSD","Zyl 8"]
["A013",null,"Narrow Band Oxygen Sensor 1","2M2 Pull Down"]
["A014",null,"Rad Fan Relay 2","1A LSD"]
["A015",null,"Lambda1 R "]
["A016",null,"Cam Return","0V"]
["A017",null,"EGT Signal","100k Pull Up"]
["A018",null,"Air Temp Signal","1k Pull Up"]
["A019",null,"Engine Oil Pressure Signal","100r Pull Up"]
["A020",null,"Shift Up Solenoid","1A LSD"]
["A021",null,"Ignition Drive E",null,"Zylinder 6"]
["A022",null,"Ignition Drive F",null,"Zylinder 3"]
["A023",null,"Ignition Drive G",null,"Zylinder 7"]
["A024",null,"Ignition Drive H",null,"Zylinder 8"]
["A025",null,"Shift Light","1A LSD"]
["A026",null,"Launch Signal","100k Pull Up"]
["A027",null,"Injector Drive C","1A LSD","Zyl 4"]
["A028",null,null,"1k Pull Up"]
["A029",null,"Lambda1 N"]
["A030",null,"5Va2","5Va2"]
["A031",null,"Injector Drive G","1A LSD","Zyl 7"]
["A032",null,"0va","0Va"]
["A033",null,null,"1A LSD"]
["A034",null,"Fuel Pressure Signal","100r Pull Up"]
["A035",null,"Cam Supply","5Va2"]
["A036",null,"MAP 2 Signal","100k Pull Down"]
["A037",null,"Powershift Signal","100k Pull Up (Digital Only)"]
["A038",null,"TPS2 Signal","100k Pull Up"]
["A039",null,null,"1A LSD"]
["A040",null,"Egas2 Motor Drive +","H Bridge"]
["A041",null,"Egas2 Motor Drive -","H Bridge"]
["A042",null,"Lambda Sensor 2 Heater","5A LS PWM"]
["A043",null,"Lambda Sensor 1 Heater","5A LS PWM"]
["A044",null,"Shift Light 2","1A LSD"]
["A045",null,"Pedal A Signal","100k Pull Up"]
["A046",null,"Injector Drive B","1A LSD","Zyl 5"]
["A047",null,"TPS1 Signal ","100k Pull Up"]
["A048",null,"Lambda1 VG"]
["A049",null,"Lambda1 P"]
["A050",null,"Injector Drive E","1A LSD","Zyl 6"]
["A051",null,"0Va","0Va"]
["A052",null,"Rad Fan Relay 1","1A LSD"]
["A053",null,"Gearbox Signal","100k Pull Up"]
["A054",null,"Cam 2 Signal","4k7 Pull Up"]
["A055",null,"Pedal B Signal","100k Pull Down"]
["A056",null,"Engine Stop Signal","100k Pull Down"]
["A057",null,"TPS4 Signal ","100k Pull Up"]
["A058",null,"Down Shift Solenoid","1A LSD"]
["A059",null,"Egas1 Motor Drive +","H Bridge"]
["A060",null,"Egas1 Motor Drive -","H Bridge"]
["A061",null,"Varable Cam 2 Drive","2A LSD PWM"]
["A062",null,"Varable Cam 1 Drive","2A LSD PWM"]
["A063",null,"Neutral Light","1A LSD"]
["A064",null,null,"1k Pull Up"]
["A065",null,"Injector Drive A","1A LSD","Zyl 1"]
["A066",null,"MAP Signal","100k Pull Down"]
["A067",null,"Water Temp Signal","1k/18k Pull Up"]
["A068",null,"Neutral Request","18k Pull Up"]
["A069",null,"Injector Drive F","1A LSD","Zyl 3"]
["A070",null,"0Va","0Va"]
["A071",null,"Throttle Blip Solenoid","1A LSD"]
["A072",null,"Narrow Band Oxygen Sensor 2","2M2 Pull Down"]
["A073",null,"Cam1 Signal","4k7 Pull Up"]
["A074",null,"TPS3 Signal ","100K Pull up"]
["A075",null,"AirPressure Input","100k Pull Down"]
["A076",null,"Nitrous Input Pin","100k Pull Up"]
["A077",null,null,"1A LSD"]
["A078",null,null,"0.5A LSD PWM"]
["A079",null,"Wastegate Drive","2A LSD PWM"]
["A080",null,"PWM Water Pump","2A LSD PWM"]
["A081",null,"Tachometer Drive","0.5A LSD PWM 1k Pull Up"]
[]
["B082",null,null,"1A LSD"]
["B083",null,"Lambda2 P"]
["B084",null,"Lambda2 R"]
["B085",null,"Knock1 Signal"]
["B086",null,"Wheelspeed 1 (FL)","4k7 Pull Up"]
["B087",null,"Wheelspeed 2 (FR)","4k7 Pull Up"]
["B088",null,"Serial TXD / CAN 2 H"]
["B089",null,"CAN H"]
["B090",null,"Fuel Pump Relay","1A LSD"]
["B091",null,"Lambda2 N"]
["B092",null,"Lambda2 VG"]
["B093",null,"Knock1 Return"]
["B094",null,"Wheelspeed 3 (RL)","4k7 Pull Up"]
["B095",null,"Wheelspeed 4 (RR)","4k7 Pull Up"]
["B096",null,"Serial RXD / CAN 2 L"]
["B097",null,"CAN L"]
["B098",null,"Engine Stop Output","1A LSD"]
["B099",null,"5Va1","5Va1"]
["B100",null,"Crank Signal"]
["B101",null,"Knock 2 Signal"]
["B102",null,"WheelSpeed1 Return","0V"]
["B103",null,"WheelSpeed2 Return","0V"]
["B104",null,"WheelSpeed3 Return","0V"]
["B105",null,"WheelSpeed4 Return","0V"]
["B106",null,"PWR Hold Relay","1A LSD"]
["B107",null,"5Va1","5Va1"]
["B108",null,"Crank Return","0V"]
["B109",null,"Knock 2 Return"]
["B110",null,"Ignition Drive A",null,"Zylinder 1"]
["B111",null,"Ignition Drive B",null,"Zylinder 5"]
["B112",null,"Ignition Drive C",null,"Zylinder 4"]
["B113",null,"Ignition Drive D",null,"Zylinder 2"]
["B114",null,"HSD Battery +","12V Perm (HSD Power)"]
["B115",null,"HSD Battery +","12V Perm (HSD Power)"]
["B116",null,"Starter Solenoid","10A HSD PWM"]
["B117",null,"Ignition Output","10A HSD PWM"]
["B118",null,"Rad Fan 1 HSD","10A HSD PWM"]
["B119",null,"Fuel Pump","10A HSD PWM"]
["B120",null,"Engine Stop Output","10A HSD PWM"]
["B121",null,"PWM Water Pump","10A HSD PWM"]
[" "]

{"sheet":"BMW V8","index":4,"n_rows":126,"n_cols":5,"rows_kept":126,"cut":false,"hidden":false,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["MBE 9A9"]
["BMW V8 1-5-4-8-7-2-6-3"]
[]
["A001",null,"Ground","GND"]
["A002",null,"Ground","GND"]
["A003",null,"ECU Permanent 12V Supply","12V MEM"]
["A004",null,"12V Switch","12V Key"]
["A005",null,"12V Switch","12V Key"]
["A006",null,"Air Charge Pump Relay","1A LSD"]
["A007",null,"Oil Temp","1k Pull Up"]
["A008",null,"Injector Drive D","1A LSD","Zyl 8"]
["A009",null,"PitLimiter","100k Pull Up"]
["A010",null,"Baro Signal","100k Pull Down"]
["A011",null,"5Va2","5Va2","EngSense"]
["A012",null,"Injector Drive H","1A LSD","Zyl 3"]
["A013",null,"Narrow Band Oxygen Sensor 1","2M2 Pull Down"]
["A014",null,"Rad Fan Relay 1","1A LSD","Lüfter Kühler"]
["A015",null,"Lambda1 R "]
["A016",null,"Cam Return","0V"]
["A017",null,"Downshift Request","100k Pull Up"]
["A018",null,"Air Temp Signal","1k Pull Up"]
["A019",null,"Engine Oil Pressure Signal","100r Pull Up"]
["A020",null,"Shift Up Solenoid","1A LSD"]
["A021",null,"Ignition Drive E",null,"Zylinder 7"]
["A022",null,"Ignition Drive F",null,"Zylinder 2"]
["A023",null,"Ignition Drive G",null,"Zylinder 6"]
["A024",null,"Ignition Drive H",null,"Zylinder 3"]
["A025",null,"Shift Light","1A LSD"]
["A026",null,"Launch Signal","100k Pull Up"]
["A027",null,"Injector Drive C","1A LSD","Zyl 4"]
["A028",null,null,"1k Pull Up"]
["A029",null,"Lambda1 N"]
["A030",null,"5Va2","5Va2","LTC"]
["A031",null,"Injector Drive G","1A LSD","Zyl 6"]
["A032",null,"0va","0Va"]
["A033",null,null,"1A LSD"]
["A034",null,"Fuel Pressure Signal","100r Pull Up"]
["A035",null,"Cam Supply","5Va2"]
["A036",null,"MAP 2 Signal","100k Pull Down"]
["A037",null,"Powershift Signal","100k Pull Up (Digital Only)"]
["A038",null,"TPS2 Signal","100k Pull Up"]
["A039",null,null,"1A LSD"]
["A040",null,"Egas2 Motor Drive -","H Bridge"]
["A041",null,"Egas2 Motor Drive +","H Bridge"]
["A042",null,"Lambda Sensor 2 Heater","5A LS PWM"]
["A043",null,"Lambda Sensor 1 Heater","5A LS PWM"]
["A044",null,"Shift Light 2","1A LSD"]
["A045",null,"Pedal A Signal","100k Pull Up"]
["A046",null,"Injector Drive B","1A LSD","Zyl 5"]
["A047",null,"TPS1 Signal ","100k Pull Up"]
["A048",null,"Lambda1 VG"]
["A049",null,"Lambda1 P"]
["A050",null,"Injector Drive E","1A LSD","Zyl 7"]
["A051",null,"0Va","0Va"]
["A052",null,"Rad Fan Relay 2","1A LSD"]
["A053",null,"Gearbox Signal","100k Pull Up"]
["A054",null,"Cam 2 Signal","4k7 Pull Up"]
["A055",null,"Pedal B Signal","100k Pull Down"]
["A056",null,"Engine Stop Signal","100k Pull Down"]
["A057",null,"TPS4 Signal ","100k Pull Up"]
["A058",null,"Down Shift Solenoid","1A LSD"]
["A059",null,"Egas1 Motor Drive -","H Bridge"]
["A060",null,"Egas1 Motor Drive +","H Bridge"]
["A061",null,"Varable Cam 2 Drive","2A LSD PWM"]
["A062",null,"Varable Cam 1 Drive","2A LSD PWM"]
["A063",null,"Neutral Light","1A LSD"]
["A064",null,"Starter Button","1k Pull Up"]
["A065",null,"Injector Drive A","1A LSD","Zyl 1"]
["A066",null,"MAP Signal","100k Pull Down"]
["A067",null,"Water Temp Signal","1k/18k Pull Up"]
["A068",null,"Neutral Request","18k Pull Up"]
["A069",null,"Injector Drive F","1A LSD","Zyl 2"]
["A070",null,"0Va","0Va"]
["A071",null,"Throttle Blip Solenoid","1A LSD"]
["A072",null,"Narrow Band Oxygen Sensor 2","2M2 Pull Down"]
["A073",null,"Cam1 Signal","4k7 Pull Up"]
["A074",null,"TPS3 Signal ","100K Pull up"]
["A075",null,"AirPressure Input","100k Pull Down"]
["A076",null,"Analog Input","100k Pull Up"]
["A077",null,null,"1A LSD"]
["A078",null,null,"0.5A LSD PWM"]
["A079",null,null,"2A LSD PWM"]
["A080",null,null,"2A LSD PWM"]
["A081",null,"Tachometer Drive","0.5A LSD PWM 1k Pull Up"]
[]
["B082",null,null,"1A LSD"]
["B083",null,"Lambda2 P"]
["B084",null,"Lambda2 R"]
["B085",null,"Knock1 Signal"]
["B086",null,"Wheelspeed 1 (FL)","4k7 Pull Up"]
["B087",null,"Wheelspeed 2 (FR)","4k7 Pull Up"]
["B088",null,"Serial TXD / CAN 2 H"]
["B089",null,"CAN H"]
["B090",null,"Fuel Pump Relay","1A LSD"]
["B091",null,"Lambda2 N"]
["B092",null,"Lambda2 VG"]
["B093",null,"Knock1 Return"]
["B094",null,"Wheelspeed 3 (RL)","4k7 Pull Up"]
["B095",null,"Wheelspeed 4 (RR)","4k7 Pull Up"]
["B096",null,"Serial RXD / CAN 2 L"]
["B097",null,"CAN L"]
["B098",null,"Generic Output 2","1A LSD"]
["B099",null,"5Va1","5Va1","TPS"]
["B100",null,"Crank Signal"]
["B101",null,"Knock 2 Signal"]
["B102",null,"WheelSpeed1 Return","0V"]
["B103",null,"WheelSpeed2 Return","0V"]
["B104",null,"WheelSpeed3 Return","0V"]
["B105",null,"WheelSpeed4 Return","0V"]
["B106",null,"PWR Hold Relay","1A LSD"]
["B107",null,"5Va1","5Va1","Pedal"]
["B108",null,"Crank Return","0V"]
["B109",null,"Knock 2 Return"]
["B110",null,"Ignition Drive A",null,"Zylinder 1"]
["B111",null,"Ignition Drive B",null,"Zylinder 5"]
["B112",null,"Ignition Drive C",null,"Zylinder 4"]
["B113",null,"Ignition Drive D",null,"Zylinder 8"]
["B114",null,"HSD Battery +","12V Perm (HSD Power)"]
["B115",null,"HSD Battery +","12V Perm (HSD Power)"]
["B116",null,"Starter Solenoid","10A HSD PWM"]
["B117",null,"Ignition Output","10A HSD PWM"]
["B118",null,"Rad Fan 1 HSD","10A HSD PWM"]
["B119",null,"Fuel Pump","10A HSD PWM"]
["B120",null,"Engine Stop Output","10A HSD PWM"]
["B121",null,"PWM Water Pump","10A HSD PWM"]
[" "]

{"sheet":"Audi I5","index":5,"n_rows":126,"n_cols":5,"rows_kept":126,"cut":false,"hidden":false,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["MBE 9A9"]
["Audi I5 1-2-4-5-3"]
[]
["A001",null,"Ground","GND"]
["A002",null,"Ground","GND"]
["A003",null,"ECU Permanent 12V Supply","12V MEM"]
["A004",null,"12V Switch","12V Key"]
["A005",null,"12V Switch","12V Key"]
["A006",null,"Air Charge Pump Relay","1A LSD"]
["A007",null,"Oil Temp","1k Pull Up"]
["A008",null,"Injector Drive D","1A LSD","Zyl 5"]
["A009",null,"Anti Lag Signal","100k Pull Up"]
["A010",null,"Baro Signal","100k Pull Down"]
["A011",null,"5Va2","5Va2"]
["A012",null,"Injector Drive H","1A LSD"]
["A013",null,"Narrow Band Oxygen Sensor 1","2M2 Pull Down"]
["A014",null,"Rad Fan Relay 2","1A LSD"]
["A015",null,"Lambda1 R "]
["A016",null,"Cam Return","0V"]
["A017",null,"EGT Signal","100k Pull Up"]
["A018",null,"Air Temp Signal","1k Pull Up"]
["A019",null,"Engine Oil Pressure Signal","100r Pull Up"]
["A020",null,"Shift Up Solenoid","1A LSD"]
["A021",null,"Ignition Drive E",null,"Zylinder 3"]
["A022",null,"Ignition Drive F"]
["A023",null,"Ignition Drive G"]
["A024",null,"Ignition Drive H"]
["A025",null,"Shift Light","1A LSD"]
["A026",null,"Launch Signal","100k Pull Up"]
["A027",null,"Injector Drive C","1A LSD","Zyl 4"]
["A028",null,null,"1k Pull Up"]
["A029",null,"Lambda1 N"]
["A030",null,"5Va2","5Va2"]
["A031",null,"Injector Drive G","1A LSD"]
["A032",null,"0va","0Va"]
["A033",null,null,"1A LSD"]
["A034",null,"Fuel Pressure Signal","100r Pull Up"]
["A035",null,"Cam Supply","5Va2"]
["A036",null,"MAP 2 Signal","100k Pull Down"]
["A037",null,"Powershift Signal","100k Pull Up (Digital Only)"]
["A038",null,"TPS2 Signal","100k Pull Up"]
["A039",null,null,"1A LSD"]
["A040",null,"Egas2 Motor Drive -","H Bridge"]
["A041",null,"Egas2 Motor Drive +","H Bridge"]
["A042",null,"Lambda Sensor 2 Heater","5A LS PWM"]
["A043",null,"Lambda Sensor 1 Heater","5A LS PWM"]
["A044",null,"Shift Light 2","1A LSD"]
["A045",null,"Pedal A Signal","100k Pull Up"]
["A046",null,"Injector Drive B","1A LSD","Zyl 2"]
["A047",null,"TPS1 Signal ","100k Pull Up"]
["A048",null,"Lambda1 VG"]
["A049",null,"Lambda1 P"]
["A050",null,"Injector Drive E","1A LSD","Zyl 3"]
["A051",null,"0Va","0Va"]
["A052",null,"Rad Fan Relay 1","1A LSD"]
["A053",null,"Gearbox Signal","100k Pull Up"]
["A054",null,"Cam 2 Signal","4k7 Pull Up"]
["A055",null,"Pedal B Signal","100k Pull Down"]
["A056",null,"Engine Stop Signal","100k Pull Down"]
["A057",null,"TPS4 Signal ","100k Pull Up"]
["A058",null,"Down Shift Solenoid","1A LSD"]
["A059",null,"Egas1 Motor Drive -","H Bridge"]
["A060",null,"Egas1 Motor Drive +","H Bridge"]
["A061",null,"Varable Cam 2 Drive","2A LSD PWM"]
["A062",null,"Varable Cam 1 Drive","2A LSD PWM"]
["A063",null,"Neutral Light","1A LSD"]
["A064",null,null,"1k Pull Up"]
["A065",null,"Injector Drive A","1A LSD","Zyl 1"]
["A066",null,"MAP Signal","100k Pull Down"]
["A067",null,"Water Temp Signal","1k/18k Pull Up"]
["A068",null,"Neutral Request","18k Pull Up"]
["A069",null,"Injector Drive F","1A LSD"]
["A070",null,"0Va","0Va"]
["A071",null,"Throttle Blip Solenoid","1A LSD"]
["A072",null,"Narrow Band Oxygen Sensor 2","2M2 Pull Down"]
["A073",null,"Cam1 Signal","4k7 Pull Up"]
["A074",null,"TPS3 Signal ","100K Pull up"]
["A075",null,"AirPressure Input","100k Pull Down"]
["A076",null,"Nitrous Input Pin","100k Pull Up"]
["A077",null,null,"1A LSD"]
["A078",null,null,"0.5A LSD PWM"]
["A079",null,"Wastegate Drive","2A LSD PWM"]
["A080",null,"PWM Water Pump","2A LSD PWM"]
["A081",null,"Tachometer Drive","0.5A LSD PWM 1k Pull Up"]
[]
["B082",null,null,"1A LSD"]
["B083",null,"Lambda2 P"]
["B084",null,"Lambda2 R"]
["B085",null,"Knock1 Signal"]
["B086",null,"Wheelspeed 1 (FL)","4k7 Pull Up"]
["B087",null,"Wheelspeed 2 (FR)","4k7 Pull Up"]
["B088",null,"Serial TXD / CAN 2 H"]
["B089",null,"CAN H"]
["B090",null,"Fuel Pump Relay","1A LSD"]
["B091",null,"Lambda2 N"]
["B092",null,"Lambda2 VG"]
["B093",null,"Knock1 Return"]
["B094",null,"Wheelspeed 3 (RL)","4k7 Pull Up"]
["B095",null,"Wheelspeed 4 (RR)","4k7 Pull Up"]
["B096",null,"Serial RXD / CAN 2 L"]
["B097",null,"CAN L"]
["B098",null,"Engine Stop Output","1A LSD"]
["B099",null,"5Va1","5Va1"]
["B100",null,"Crank Signal"]
["B101",null,"Knock 2 Signal"]
["B102",null,"WheelSpeed1 Return","0V"]
["B103",null,"WheelSpeed2 Return","0V"]
["B104",null,"WheelSpeed3 Return","0V"]
["B105",null,"WheelSpeed4 Return","0V"]
["B106",null,"PWR Hold Relay","1A LSD"]
["B107",null,"5Va1","5Va1"]
["B108",null,"Crank Return","0V"]
["B109",null,"Knock 2 Return"]
["B110",null,"Ignition Drive A",null,"Zylinder 1"]
["B111",null,"Ignition Drive B",null,"Zylinder 2"]
["B112",null,"Ignition Drive C",null,"Zylinder 4"]
["B113",null,"Ignition Drive D",null,"Zylinder 5"]
["B114",null,"HSD Battery +","12V Perm (HSD Power)"]
["B115",null,"HSD Battery +","12V Perm (HSD Power)"]
["B116",null,"Starter Solenoid","10A HSD PWM"]
["B117",null,"Ignition Output","10A HSD PWM","LA Power"]
["B118",null,"Rad Fan 1 HSD","10A HSD PWM"]
["B119",null,"Fuel Pump","10A HSD PWM"]
["B120",null,"Engine Stop Output","10A HSD PWM"]
["B121",null,"PWM Water Pump","10A HSD PWM"]
[" "]

{"sheet":"BMW V8 VANOS","index":6,"n_rows":126,"n_cols":5,"rows_kept":126,"cut":false,"hidden":false,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["MBE 9A9"]
["BMW V8 1-5-4-8-7-2-6-3"]
[]
["A001",null,"Ground","GND"]
["A002",null,"Ground","GND"]
["A003",null,"ECU Permanent 12V Supply","12V MEM"]
["A004",null,"12V Switch","12V Key"]
["A005",null,"12V Switch","12V Key"]
["A006",null,"Air Charge Pump Relay","1A LSD"]
["A007",null,"Oil Temp","1k Pull Up"]
["A008",null,"Injector Drive D","1A LSD","Zyl 8"]
["A009",null,"PitLimiter","100k Pull Up"]
["A010",null,"Baro Signal","100k Pull Down"]
["A011",null,"5Va2","5Va2"]
["A012",null,"Injector Drive H","1A LSD","Zyl 3"]
["A013",null,"Narrow Band Oxygen Sensor 1","2M2 Pull Down"]
["A014",null,"Rad Fan Relay 1","1A LSD"]
["A015",null,"Lambda1 R "]
["A016",null,"Cam Return","0V"]
["A017",null,"Downshift Request","100k Pull Up"]
["A018",null,"Air Temp Signal","1k Pull Up"]
["A019",null,"Engine Oil Pressure Signal","100r Pull Up"]
["A020",null,"Shift Up Solenoid","1A LSD"]
["A021",null,"Ignition Drive E",null,"Zylinder 7"]
["A022",null,"Ignition Drive F",null,"Zylinder 2"]
["A023",null,"Ignition Drive G",null,"Zylinder 6"]
["A024",null,"Ignition Drive H",null,"Zylinder 3"]
["A025",null,"Shift Light","1A LSD"]
["A026",null,"Launch Signal","100k Pull Up"]
["A027",null,"Injector Drive C","1A LSD","Zyl 4"]
["A028",null,null,"1k Pull Up"]
["A029",null,"Lambda1 N"]
["A030",null,"5Va2","5Va2"]
["A031",null,"Injector Drive G","1A LSD","Zyl 6"]
["A032",null,"0va","0Va"]
["A033",null,null,"1A LSD"]
["A034",null,"Fuel Pressure Signal","100r Pull Up"]
["A035",null,"Cam Supply","5Va2"]
["A036",null,"MAP 2 Signal","100k Pull Down"]
["A037",null,"Powershift Signal","100k Pull Up (Digital Only)"]
["A038",null,"TPS2 Signal","100k Pull Up"]
["A039",null,null,"1A LSD"]
["A040",null,"Egas2 Motor Drive -","H Bridge"]
["A041",null,"Egas2 Motor Drive +","H Bridge"]
["A042",null,"Lambda Sensor 2 Heater","5A LS PWM"]
["A043",null,"Lambda Sensor 1 Heater","5A LS PWM"]
["A044",null,"Shift Light 2","1A LSD"]
["A045",null,"Pedal A Signal","100k Pull Up"]
["A046",null,"Injector Drive B","1A LSD","Zyl 5"]
["A047",null,"TPS1 Signal ","100k Pull Up"]
["A048",null,"Lambda1 VG"]
["A049",null,"Lambda1 P"]
["A050",null,"Injector Drive E","1A LSD","Zyl 7"]
["A051",null,"0Va","0Va"]
["A052",null,"Rad Fan Relay 2","1A LSD"]
["A053",null,"Gearbox Signal","100k Pull Up"]
["A054",null,"Cam 2 Signal","4k7 Pull Up","EX1-4"]
["A055",null,"Pedal B Signal","100k Pull Down"]
["A056",null,"Engine Stop Signal","100k Pull Down"]
["A057",null,"TPS4 Signal ","100k Pull Up"]
["A058",null,"Down Shift Solenoid","1A LSD"]
["A059",null,"Egas1 Motor Drive -","H Bridge"]
["A060",null,"Egas1 Motor Drive +","H Bridge"]
["A061",null,"Varable Cam 2 Drive","2A LSD PWM","EX1-4"]
["A062",null,"Varable Cam 1 Drive","2A LSD PWM","IN1-4"]
["A063",null,"Neutral Light","1A LSD"]
["A064",null,"Starter Button","1k Pull Up"]
["A065",null,"Injector Drive A","1A LSD","Zyl 1"]
["A066",null,"MAP Signal","100k Pull Down"]
["A067",null,"Water Temp Signal","1k/18k Pull Up"]
["A068",null,"Neutral Request","18k Pull Up"]
["A069",null,"Injector Drive F","1A LSD","Zyl 2"]
["A070",null,"0Va","0Va"]
["A071",null,"Throttle Blip Solenoid","1A LSD"]
["A072",null,"Narrow Band Oxygen Sensor 2","2M2 Pull Down"]
["A073",null,"Cam1 Signal","4k7 Pull Up","IN1-4"]
["A074",null,"TPS3 Signal ","100K Pull up"]
["A075",null,"AirPressure Input","100k Pull Down"]
["A076",null,"Analog Input","100k Pull Up"]
["A077",null,null,"1A LSD"]
["A078",null,null,"0.5A LSD PWM"]
["A079",null,"Varable Cam 3 Drive","2A LSD PWM","IN5-8"]
["A080",null,"Varable Cam 4 Drive","2A LSD PWM","EX5-8"]
["A081",null,"Tachometer Drive","0.5A LSD PWM 1k Pull Up"]
[]
["B082",null,null,"1A LSD"]
["B083",null,"Lambda2 P"]
["B084",null,"Lambda2 R"]
["B085",null,"Knock1 Signal"]
["B086",null,"Wheelspeed 1 (FL)","4k7 Pull Up"]
["B087",null,"Wheelspeed 2 (FR)","4k7 Pull Up"]
["B088",null,"Serial TXD / CAN 2 H"]
["B089",null,"CAN H"]
["B090",null,"Fuel Pump Relay","1A LSD"]
["B091",null,"Lambda2 N"]
["B092",null,"Lambda2 VG"]
["B093",null,"Knock1 Return"]
["B094",null,"CAM3","4k7 Pull Up","IN5-8"]
["B095",null,"CAM4","4k7 Pull Up","EX5-8"]
["B096",null,"Serial RXD / CAN 2 L"]
["B097",null,"CAN L"]
["B098",null,"Generic Output 2","1A LSD"]
["B099",null,"5Va1","5Va1"]
["B100",null,"Crank Signal"]
["B101",null,"Knock 2 Signal"]
["B102",null,"WheelSpeed1 Return","0V"]
["B103",null,"WheelSpeed2 Return","0V"]
["B104",null,"CAM3 Return","0V"]
["B105",null,"CAM4 Return","0V"]
["B106",null,"PWR Hold Relay","1A LSD"]
["B107",null,"5Va1","5Va1"]
["B108",null,"Crank Return","0V"]
["B109",null,"Knock 2 Return"]
["B110",null,"Ignition Drive A",null,"Zylinder 1"]
["B111",null,"Ignition Drive B",null,"Zylinder 5"]
["B112",null,"Ignition Drive C",null,"Zylinder 4"]
["B113",null,"Ignition Drive D",null,"Zylinder 8"]
["B114",null,"HSD Battery +","12V Perm (HSD Power)"]
["B115",null,"HSD Battery +","12V Perm (HSD Power)"]
["B116",null,"Starter Solenoid","10A HSD PWM"]
["B117",null,"Ignition Output","10A HSD PWM"]
["B118",null,"Rad Fan 1 HSD","10A HSD PWM"]
["B119",null,"Fuel Pump","10A HSD PWM"]
["B120",null,"Engine Stop Output","10A HSD PWM"]
["B121",null,"PWM Water Pump","10A HSD PWM"]
[" "]

{"sheet":"Audi V8","index":7,"n_rows":126,"n_cols":5,"rows_kept":126,"cut":false,"hidden":false,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["MBE 9A9"]
["Audi V8 1-5-4-8-6-3-7-2"]
[]
["A001",null,"Ground","GND"]
["A002",null,"Ground","GND"]
["A003",null,"ECU Permanent 12V Supply","12V MEM"]
["A004",null,"12V Switch","12V Key"]
["A005",null,"12V Switch","12V Key"]
["A006",null,"Air Charge Pump Relay","1A LSD"]
["A007",null,"Oil Temp","1k Pull Up"]
["A008",null,"Injector Drive D","1A LSD","Zyl 8"]
["A009",null,"PitLimiter","100k Pull Up"]
["A010",null,"Baro Signal","100k Pull Down"]
["A011",null,"5Va2","5Va2","EngSense"]
["A012",null,"Injector Drive H","1A LSD","Zyl 2"]
["A013",null,"Narrow Band Oxygen Sensor 1","2M2 Pull Down"]
["A014",null,"Rad Fan Relay 1","1A LSD","Lüfter Kühler"]
["A015",null,"Lambda1 R "]
["A016",null,"Cam Return","0V"]
["A017",null,"Downshift Request","100k Pull Up"]
["A018",null,"Air Temp Signal","1k Pull Up"]
["A019",null,"Engine Oil Pressure Signal","100r Pull Up"]
["A020",null,"Shift Up Solenoid","1A LSD"]
["A021",null,"Ignition Drive E",null,"Zylinder 6"]
["A022",null,"Ignition Drive F",null,"Zylinder 3"]
["A023",null,"Ignition Drive G",null,"Zylinder 7"]
["A024",null,"Ignition Drive H",null,"Zylinder 2"]
["A025",null,"Shift Light","1A LSD"]
["A026",null,"Launch Signal","100k Pull Up"]
["A027",null,"Injector Drive C","1A LSD","Zyl 4"]
["A028",null,null,"1k Pull Up"]
["A029",null,"Lambda1 N"]
["A030",null,"5Va2","5Va2","LTC"]
["A031",null,"Injector Drive G","1A LSD","Zyl 7"]
["A032",null,"0va","0Va"]
["A033",null,null,"1A LSD"]
["A034",null,"Fuel Pressure Signal","100r Pull Up"]
["A035",null,"Cam Supply","5Va2"]
["A036",null,"MAP 2 Signal","100k Pull Down"]
["A037",null,"Powershift Signal","100k Pull Up (Digital Only)"]
["A038",null,"TPS2 Signal","100k Pull Up"]
["A039",null,null,"1A LSD"]
["A040",null,"Egas2 Motor Drive -","H Bridge"]
["A041",null,"Egas2 Motor Drive +","H Bridge"]
["A042",null,"Lambda Sensor 2 Heater","5A LS PWM"]
["A043",null,"Lambda Sensor 1 Heater","5A LS PWM"]
["A044",null,"Shift Light 2","1A LSD"]
["A045",null,"Pedal A Signal","100k Pull Up"]
["A046",null,"Injector Drive B","1A LSD","Zyl 5"]
["A047",null,"TPS1 Signal ","100k Pull Up"]
["A048",null,"Lambda1 VG"]
["A049",null,"Lambda1 P"]
["A050",null,"Injector Drive E","1A LSD","Zyl 6"]
["A051",null,"0Va","0Va"]
["A052",null,"Rad Fan Relay 2","1A LSD"]
["A053",null,"Gearbox Signal","100k Pull Up"]
["A054",null,"Cam 2 Signal","4k7 Pull Up"]
["A055",null,"Pedal B Signal","100k Pull Down"]
["A056",null,"Engine Stop Signal","100k Pull Down"]
["A057",null,"TPS4 Signal ","100k Pull Up"]
["A058",null,"Down Shift Solenoid","1A LSD"]
["A059",null,"Egas1 Motor Drive -","H Bridge"]
["A060",null,"Egas1 Motor Drive +","H Bridge"]
["A061",null,"Varable Cam 2 Drive","2A LSD PWM"]
["A062",null,"Varable Cam 1 Drive","2A LSD PWM"]
["A063",null,"Neutral Light","1A LSD"]
["A064",null,"Starter Button","1k Pull Up"]
["A065",null,"Injector Drive A","1A LSD","Zyl 1"]
["A066",null,"MAP Signal","100k Pull Down"]
["A067",null,"Water Temp Signal","1k/18k Pull Up"]
["A068",null,"Neutral Request","18k Pull Up"]
["A069",null,"Injector Drive F","1A LSD","Zyl 3"]
["A070",null,"0Va","0Va"]
["A071",null,"Throttle Blip Solenoid","1A LSD"]
["A072",null,"Narrow Band Oxygen Sensor 2","2M2 Pull Down"]
["A073",null,"Cam1 Signal","4k7 Pull Up"]
["A074",null,"TPS3 Signal ","100K Pull up"]
["A075",null,"AirPressure Input","100k Pull Down"]
["A076",null,"Analog Input","100k Pull Up"]
["A077",null,null,"1A LSD"]
["A078",null,null,"0.5A LSD PWM"]
["A079",null,null,"2A LSD PWM"]
["A080",null,null,"2A LSD PWM"]
["A081",null,"Tachometer Drive","0.5A LSD PWM 1k Pull Up"]
[]
["B082",null,null,"1A LSD"]
["B083",null,"Lambda2 P"]
["B084",null,"Lambda2 R"]
["B085",null,"Knock1 Signal"]
["B086",null,"Wheelspeed 1 (FL)","4k7 Pull Up"]
["B087",null,"Wheelspeed 2 (FR)","4k7 Pull Up"]
["B088",null,"Serial TXD / CAN 2 H"]
["B089",null,"CAN H"]
["B090",null,"Fuel Pump Relay","1A LSD"]
["B091",null,"Lambda2 N"]
["B092",null,"Lambda2 VG"]
["B093",null,"Knock1 Return"]
["B094",null,"Wheelspeed 3 (RL)","4k7 Pull Up"]
["B095",null,"Wheelspeed 4 (RR)","4k7 Pull Up"]
["B096",null,"Serial RXD / CAN 2 L"]
["B097",null,"CAN L"]
["B098",null,"Generic Output 2","1A LSD"]
["B099",null,"5Va1","5Va1","TPS"]
["B100",null,"Crank Signal"]
["B101",null,"Knock 2 Signal"]
["B102",null,"WheelSpeed1 Return","0V"]
["B103",null,"WheelSpeed2 Return","0V"]
["B104",null,"WheelSpeed3 Return","0V"]
["B105",null,"WheelSpeed4 Return","0V"]
["B106",null,"PWR Hold Relay","1A LSD"]
["B107",null,"5Va1","5Va1","Pedal"]
["B108",null,"Crank Return","0V"]
["B109",null,"Knock 2 Return"]
["B110",null,"Ignition Drive A",null,"Zylinder 1"]
["B111",null,"Ignition Drive B",null,"Zylinder 5"]
["B112",null,"Ignition Drive C",null,"Zylinder 4"]
["B113",null,"Ignition Drive D",null,"Zylinder 8"]
["B114",null,"HSD Battery +","12V Perm (HSD Power)"]
["B115",null,"HSD Battery +","12V Perm (HSD Power)"]
["B116",null,"Starter Solenoid","10A HSD PWM"]
["B117",null,"Ignition Output","10A HSD PWM"]
["B118",null,"Rad Fan 1 HSD","10A HSD PWM"]
["B119",null,"Fuel Pump","10A HSD PWM"]
["B120",null,"Engine Stop Output","10A HSD PWM"]
["B121",null,"PWM Water Pump","10A HSD PWM"]
[" "]